

**A10 Snow Guard Specification Sheet**

***PART 1 GENERAL***

* 1. SUMMARY

1. Work Includes

1. Install A10 Snow Guard to roof system.

2. Provide necessary components: A10 Snow Guard and Fasteners (3 #12 Screws or 5 Nails).

1.2 RELATED SECTIONS

1. Section 07310 Roofing Shingles

2. Section 07600 Flashing and Sheet Metal

3. Division 7: Thermal and Moisture Protection

1.3 SYSTEM

1. Components

1. A10 Snow Guard.

2. Fasteners.

1. Design - To be recommended by Manufacturer or Structural Engineer.

1.4 SUBMITTAL - Submit Manufacturers Specifications, recommended layout, product drawings and installation instructions.

1.5 QUALITY ASSURANCE - Installer to be experienced in roofing and snow retention for a minimum of not less than 5 years.

1.6 DELIVERY/STORAGE - Inspect material upon delivery and inform distributer of any damaged or missing items. Protect materials from damage until installation.

***PART 2 PRODUCTS***

2.1 MANUFACTURER

A. Ice Control Engineering, Inc. - 122 N. 1800 W. Unit #9. Lindon, Utah 84042

Tel. (801) 787-6555; Email: icecontrol@comcast.net; Web: www.icesnowguards.com

2.2 MATERIALS

A. A10 Snow Guard 14 gauge electro galvanized steel.

B. Fasteners 2” zinc plated #12 screws or 2” zinc plated ring shank roofing nail.

2.3 FINISH - TGIC Polyester powder coating

***PART 3 EXECUTION***

3.1 EXAMINATION - Inspect roof structure and panel attachment to insure it will withstand snow loads. Correct all problems before installation of snow fence.

3.2 INSTALLATION - Install according to architects drawing and manufacturer’s instructions.